2007/06/26 Wrote by Kidd Wang.
T60H976.00 XB63 Released for xp-32/64bits: 
1.WHQL driver v5.3.0.56.(Negative-Pole LED)
  Silent insatllation: c:\Atheros-driver\setup /s or double click this file(SilentInstall.bat).
2.Update to IS12 to fix unclean remove oem*.inf issue.
3.NDIS: Remove MTU from device manager as it can cause security failure for changing the MTU size. It is left in driver for         debugging only.
4.NDIS: Fixed, can not pass data in some networks even if the wireless security passes and ping data passes. This issue is         because there was a shift in the tid by 4 bits for crypto check of received frames. Shift is required only for data         frame receive path and not tid.
